**Part Number: EA1-B0-16-680-32A-BF**

* E SERIES HYDRAULIC/MAGNETIC CIRCUIT BREAKER
* HANDLE ACTUATOR (ONE PER POLE)
* ONE POLE CIRCUIT BREAKER
* SERIES TRIP (CURRENT COIL)
* NO AUXILIARY SWITCH SUPPLIED
* DELAY CURVE: DC LONG
* CURRENT TRIP RATING GREATER THAN 50 AMPS
* NON-STANDARD CURRENT TRIP RATING: 80 AMP
* TERMINAL: FRONT CONNECTED (BACK MOUNT ONLY)
* BOX WIRE CONNECTOR (LINE & LOAD)
* MAXIMUM RATING FOR TERMINAL CHOICE: 100 AMPS
* ACTUATOR COLOR: BLACK; I-O & ON-OFF (DUAL) LEGEND IN WHITE
* FRONT MOUNTING INSERTS (BACK CONNECTED ONLY) 6-32 MOUNTING
* MAXIMUM APPL. RATING: VOLTAGE 125VDC; CURRENT 100 AMPS
* UL 489 LISTED, CSA CERTIFIED
* VDE CERTIFIED